**Specifications:**

**1.Topfabric:**Heavy-duty 285gsm cotton canvaswith 3000mm waterproof PU coating, color of beige.(Breathable and durablecotton canvas 285g per sqm, with reinforced double stitched seams)(60cm walls can be unzipped and rolled up for airflow)

**2.Ground-sheet:**extrathick floor mat with 540gsm PVC with 5000mm waterproof PU, color of brown. (It is detachable and connectedwith sidewall by zipper, the  bell tents come with zipped In groundsheet. )

**3.CentralPole:**Spring-loaded diameter 38mm x 1.2mmgalvanized steel tube.( Black rubber gasket at both end) (Centre pole has a loopto hang chandeliers.)

**4.Door pole:**Diameter19mmx1mm galvanized steel tubes. (with a rain cap)

**5.Windows:**4 zippedroundwindows for airflow and ventilation with mesh cover to keep insects away.

**6.Door:**1 PCdoor complete with integrated mosquitoscreens and cotton canvas cover.(Secondary zipped mosquito door)

**7.Zipper:**Double-sided zippers. 3 way zips with loops that can be easily padlocked for extra security.

**8.Mosquito screen:**B3 mesh, both door and windows are equiped.

**9.Carrybag:**All packs down into a matching canvasbag small enough to go on the back of a motorbike or in a small trunk.

**10.Stitchment:**Doublestitching all around and reinforced key points.

**11.Assemble:**Takes1person only 15minutes to pitch.

**12.Accommodation:**4mcan fit 4-5 person.（can place2 Queen size bed, or 1Queen size bed with 2 single size bed)

**13.Vents:**4PCSvents to circulating air.

**Parameters:**

Item:400x400x250cm/60cm

Diameter:4m

Topheight: 250cm

Doorheight: 150cm

Sidewallheight: 60cm

Grossweight: 28kg

Guy ropes & pegs:12pcs & 24 pcs(12 small pegs and 12 large pegs)

Chimney hole: 1PC( on the sidewall)

Package size: 100x29x29cm