**Specification:**

**1.Top fabric:** Heavy-duty 285gsm cotton canvas with 3000mm waterproof PU coating, color of beige.

(Breathable and durable cotton canvas 285g per sqm, with reinforced double stitched seams)

(Remark: the sidewall of touareg tent can not be rolled up)

**2.Ground-sheet**: extra thick floor mat with 540gsm PVC with 5000mm waterproof PU, color of brown.

(It is detachable and connected with sidewall by zipper, the touareg tent come with zipped In groundsheet. )

**3.Central Pole:** Spring-loaded dia38 mm and 1.0mm thickness galvanized steel tube, .( Black rubber gasket at the top)

(Centre pole has a loop to hang chandeliers.)

**4.Door pole:**dia20mm and 1.0mm thickness galvanized steel tubes.

**5.Windows:**4 pcs triangle shape windows for airflow and ventilation with mesh cover to keep insects away.(2 pcs on backside and 2pcs on frontside)

**6.Door:**2 pcs door complete with integrated mosquito screens and cotton canvas cover.  (Secondary zipped mosquito door)

**7.Zipper:**Double-sided zippers. 3 way zips with loops that can be easily padlocked for extra security.

**8.Mosquito screen:**B3  mesh, both door and windows are equiped.

**9.Carry bag:** All packs down into a matching canvas bag .

**10.Stitchment:**Double stitching all around and reinforced key points.

**11.Assemble:** Takes 1-2 person 30 minutes to pitch.

**12.Accommodation:** 6-8 person

**Parameter:**

**Item:** Touareg tent

**Size:** 5m(L)X4m(W)x3m(H)

**Top height:** 300cm

**Door height:** 190cm

**Sidewall height:** 80cm

**Guy ropes & pegs:** 14pcs & 28 pcs(14 small pegs and 14 large pegs)

**Chimney hole:** unavailable

**Package size:** 112x32x31cm & 43kg